# Advanced Framework for Sap Flow Data Post-Process

## Documentation for package ‘fluxfixer’ version 1.1.0

- DESCRIPTION file.
- User guides, package vignettes and other documentation.
- Package NEWS.

## Help Pages

calc_dtmax | Calculate dTmax by various methods
calc_fd | Calculate sap flux density time series
calc_ref_stats | Define reference values of average and standard deviation
calc_sw_in_toa | Calculate global solar radiation time series at TOA
check_absolute_limits | Remove outliers by absolute limits
dtmax | dTmax time series estimated by multiple methods
dt_gf | Quality-controlled and gap-filled dT time series
dt_noisy | Raw dT time series with various artifacts
fill_gaps | Fill missing values with a random forest model
filter_highfreq_noise | Filter high frequency noise by Gaussian filter
interpret_qc | Convert the decimal QC flag into a human-interpretable 10-digit binary
modify_short_drift | Modify short-term drifts
remove_manually | Remove error values manually
remove_rf_outlier | Remove outliers detected by a random forest model
remove_zscore_outlier | Remove outliers by Z-score time series
retrieve_ts | Retrieve time series in its original units
run_fluxfixer | Run all quality control processes automatically